Odometer Reset key   
key switch

5V/3.3V USB   
power adapter

Processor 2

*ATmega328*

Display

*ILI9340*

Speaker   
piezzo

Blinkers control   
key switches

Speedo control   
potentiometer

t\* sensor   
DS18B20

Processor 1

*ATmega328*

* SR1 covered with Display ILI9340 – color
* SR2 covered with 2 processors ATmega328
* SR4 covered with piezzo speaker and blinker key switches.
* SR6 covered with t\* sensor DS18B20
* SR7 covered with analog input – speedo control potentiometer